For 1990-2009 cars

### Removal Procedure

Important:

• | The rear window reveal molding cannot be replaced without removing the rear window.

• | When replacing the rear window, the original rear window reveal molding cannot be reused and must be replaced with a new molding.

• | New rear window reveal moldings are primed and will adhere to the urethane adhesive.

• | Dry fit the reveal molding to the rear window and then as an assembly on the body prior to the actual installation.

• | A heat lamp may be used in order to make the rear window reveal molding more pliable.

1. Using a flat-bladed tool, carefully pry out the end of the rear window reveal molding approximately 75 mm (3 in).
2. Grasp the rear window reveal molding (1).

Slowly pull the rear window reveal molding away from the body.

3. Remove the rear window. Refer to Rear Window Replacement .

### Installation Procedure

1. Install the rear window reveal molding (1).
2. Wipe the rear window area with a clean, dampened cloth using GM Window Cleaner GM P/N 1050427 or isopropyl alcohol in order to clean the surface of the rear window for the installation of the new rear window reveal molding.

Allow to air dry.

3. Starting in the center, work outward, hand pressing the molding into place.
4. Apply tape if needed, in order to keep the rear window reveal molding on the rear window.
5. Dry fit the service molding and the rear window to the body as an assembly prior to the actual installation.
6. Install the rear window. Refer to Rear Window Replacement .