For 1990-2009 cars

## Side Marker Lamp Bulb Replacement Front

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Access the bulb socket from under the front fascia to remove the bulb socket from the front sidemarker lamp.
3. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket.
2. Install the bulb socket to the front sidemarker lamp from under the front fascia.
3. Lower the vehicle.

## Side Marker Lamp Bulb Replacement Rear

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear sidemarker lamp from the rear fascia. Refer to Side Marker Lamp Replacement
3. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket.
2. Install the rear sidemarker lamp to the rear fascia. Refer to Side Marker Lamp Replacement
3. Lower the vehicle.