For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rubber protective cover from the fog and cornering lamp.
3. Separate the bulb fastening tangs.
4. Carefully remove the bulb.
5. Remove the electrical connection from the bulb.

### Installation Procedure

1. Install the electrical connection to the bulb.
2. Snap the fastening tangs in place to install the bulb.
3. Install the rubber protective cover to the fog and cornering lamp.
4. Lower the vehicle.