For 1990-2009 cars

### Removal Procedure

1. Remove the front grille. Refer to Grille Replacement in Exterior Trim.
2. Disconnect the washer pump electrical connector.
3. Remove the washer pump from the solvent container.
4. Remove the washer pump hose from the washer pump.
5. Remove the washer pump filter from the solvent container.
6. Inspect the washer pump filter. Clean or replace as needed.

### Installation Procedure

1. Install the washer pump filter.
2. Install the washer pump hose to the washer pump.
3. Install the washer pump to the solvent container.
4. Connect the washer pump electrical connector.
5. Install the front grille. Refer to Grille Replacement in Exterior Trim.