For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seat back cushion cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Unhook lateral release cable from lateral release lever.
4. Remove lateral release lever from recliner mechanism.
5. Unroute lateral release cable form seat back frame.

### Installation Procedure

1. Route lateral release cable to seat back frame.
2. Install lateral release lever to recliner mechanism.
3. Install lateral release cable to lateral release lever.
4. Install front seat back cushion cover. Refer to Front Seat Back Cushion Cover Replacement .
5. Install front seat. Refer to Seat Replacement .