For 1990-2009 cars

### Removal Procedure

Caution: Disconnect the power window switch when working inside the driver door. When operated, the Express Up/Down Feature allows the door window to move very quickly, without stopping, which could cause personal injury.

1. Lower the window to the bottom of the door.
2. Remove front door assist handle and molding. Refer to Assist Handle and Molding Replacement - Front Door .
3. Remove the outside rearview mirror. Refer to Power Mirror Replacement .
4. Pull up on the front edge of the outer belt sealing strip in order to remove from the flange.

### Installation Procedure

1. Install the outer belt sealing strip.
2. Raise the window all the way up.
3. Install the outside rearview mirror. Refer to Power Mirror Replacement .
4. Install front door assist handle and molding. Refer to Assist Handle and Molding Replacement - Front Door .