For 1990-2009 cars

### Removal Procedure

1. Pull back the air inlet grille sealing strip.
2. Open the air inlet grille.
3. Disconnect the manifold vacuum line.
4. Disconnect the HVAC supply vacuum line.
5. Remove the vacuum tank screws.
6. Remove the vacuum tank.

### Installation Procedure

1. Install the vacuum tank.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the vacuum tank screws.

Tighten
Tighten the screws to 3.5 N·m (31 lb in).

3. Connect the HVAC supply vacuum line.
4. Connect the manifold vacuum line.
5. Close the air inlet grille.
6. Install the air inlet grille sealing strip.