For 1990-2009 cars

### Removal Procedure

1. Remove the screws (1) from the sunshade and the vanity mirror support.
2. Disconnect the electrical connector (2) from the sunshade and the vanity mirror (if equipped).
3. Remove the sunshade and the vanity mirror (3).

### Installation Procedure

1. Install the electrical connector (2) to sunshade and the vanity mirror (3) (if equipped).
2. Install the sunshade and the vanity mirror (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws (1) to the sunshade and the vanity mirror support.

Tighten
Tighten the sunshade and the vanity mirror support screw to 1.9 N·m (17 lb in).