For 1990-2009 cars

### Removal Procedure

1. Remove the hood insulator. Refer to Hood Insulator Replacement in Body Front End.
2. Remove the hose from the nozzle.
3. Disconnect the nozzle harness connector.
4. Press together the nozzle retaining tabs in order to remove the nozzle from the hood.
5. Remove the nozzle (1).

### Installation Procedure

1. Fully seat the nozzle (1) in the hood while ensuring that the retaining tabs expand.
2. Connect the nozzle harness connector.
3. Install the hose to the nozzle.
4. Install the hood insulator. Refer to Hood Insulator Replacement in Body Front End.