For 1990-2009 cars

Table 1: | Ignition Switch and Lifting Magnet
Table 2: | Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module
Table 3: | Inflatable Restraint Steering Wheel Module Coil

#### Ignition Switch and Lifting Magnet

Connector Part Information | ZF6-5
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRN | A905 | B+ from fuse #24
2 | GRN | U900 | Brake to shift signal
U | BRN | X826 | B+ in the ON position
V | BRN | X1 | B+ in the ON or START position
W | RED | A19 | B+ when the key is inserted
Y | RED | A503 | B+ form fuse V2
Z | BLK/RED | FA700 | Starter solenoid signal

#### Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module

Connector Part Information | 0688450101
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | YEL/WHT | BM30 | Driver frontal high signal
2 | YEL | B30 | Driver frontal low signal
3 | YEL/RED | BA10 | Passenger frontal low signal
4 | YEL/BLU | BP10 | Passenger frontal high signal
5 | BRN | X30 | IGN
6 | BRN/YEL | XB20 | Inflatable restraint indicator
7 | BLK | F108 | Ground to G103
8 | RED/WHT | AM900 | Driver belt high signal
9 | BRN/WHT | XM901 | Driver belt low signal
10 | BRN/YEL | XB100 | CIRCUIT NOT USED
11 | RED/YEL | AB11 | CIRCUIT NOT USED
12 | BRN/WHT | XM10 | Serial data
13 | RED/WHT | AM13 | CIRCUIT NOT USED
14 | BRN/WHT | XM14 | CIRCUIT NOT USED
15 | BRN/YEL | XB901 XB905 | Passenger belt low signal
16-40 | -- | -- | CIRCUITS NOT USED
41 | YEL | B41 | CIRCUIT NOT USED
42 | BRN/YEL | XB42 | CIRCUIT NOT USED
43 | BRN/WHT | XM430 | CIRCUIT NOT USED
44 | WHT | M44 | CIRCUIT NOT USED
45 | RED/YEL | AB900 AB950 | Passenger belt high signal

#### Inflatable Restraint Steering Wheel Module Coil

Connector Part Information | ZF 8-5
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | F122 | Ground to G201
2 | BRN/WHT | XM1 | Horn relay control signal
3 | RED/WHT | AM116 | LED control signal
4 | BLU/RED | PA101 | Steering wheel switch signal
5-6 | -- | -- | Not used
7 | YEL/WHT | BM 30 | Driver front airbag high signal
8 | YEL | B30 | Driver front airbag low signal