For 1990-2009 cars

### Removal Procedure

Important: Be sure the vehicle is level during this entire procedure.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.

Important: Due to the internal baffling in the oil pan, allow at least 5 minutes for sufficient time for oil drainage once the oil pan drain plug is removed.

2. Remove the oil pan drain plug and allow the oil to drain.

Important: To minimize oil spillage when removing the oil filter cartridge, allow sufficient time for oil drainage once the oil filter drain plug is removed.

3. Remove the oil filter drain plug and allow the oil to drain.

Important: Use a cap-type or strap-type wrench to prevent damage during removal.

4. Remove the plastic cap (3) from the oil filter cartridge housing (1).
5. Remove the oil filter cartridge (2) from the plastic cap.
6. Wipe the plastic cap and the oil filter cartridge housing with a clean, dry cloth.
7. If removing the oil filter cartridge housing from the engine block, use a socket on the sleeve (1) on the inside of the housing.

### Installation Procedure

1. If removed, install the oil filter housing to the engine block.

Tighten
Tighten the oil filter housing at the sleeve (1) to 45 N·m (33 lb ft).

2. Install the oil filter drain plug.

Tighten
Tighten the oil filter drain plug to 10 N·m (89 lb in).

Important: Ensure the tabs (1) on the oil filter cartridge lock firmly into the plastic cap.

An audible snap will be heard when the oil filter cartridge is completely seated.
3. Install the new oil filter cartridge into the plastic cap.
4. Lightly coat the O-ring (2) around the plastic cap with clean oil.

Important: Use a cap-type or strap-type wrench to prevent damage during installation.

5. Install the plastic cap (3) onto the oil filter cartridge housing (1).

Tighten
Tighten the plastic cap (3) to 25 N·m (18 lb ft).

6. Wipe the oil pan drain plug and surrounding area with a clean, dry cloth.
7. Install the oil pan drain plug.

Tighten
Tighten the oil pan drain plug to 10 N·m (89 lb in).

8. Lower the vehicle.
9. Fill the engine with the proper type and amount of engine oil. Refer to Fluid and Lubricant Recommendations and Approximate Fluid Capacities in Maintenance and Lubrication.

Important: To prevent engine damage, shut the engine off if it does not build up sufficient oil pressure within 5 seconds.

10. Start the engine and inspect the oil pressure gauge for appropriate pressure build up.
11. Inspect the oil filter and the oil pan drain plug areas for leaks.
12. Shut the engine off.
13. Inspect the engine oil level and adjust if necessary.