For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the carpet on left side (1).

Pull the carpet back in order to expose the relay location.

3. Remove the heating element relay (1) from the rear seat cushion:

• | The relays for the rear seat heating elements are located under the rear seat on left side.

• | Insert a small screwdriver into the clip on the relay to release the clip.

### Installation Procedure

1. Install the heating element relay to the rear seat cushion.

Install the relay back to its original location in order to prevent damage when installing the rear seat cushion.

2. Install the carpet on the left side.

Insert the carpet back to its original location.

3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .