For 1990-2009 cars

### Removal Procedure

1. Move the front seat to the full forward position.
2. Remove the seatback panel screws.
3. Remove the seatback panel from the seatback.

### Installation Procedure

1. Install the seatback panel to the seatback.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seatback panel screws.

Tighten
Tighten the seatback panel screws until fully seated and not stripped.

3. Install the front seat to the original position.