For 1990-2009 cars

Table 1: | Hose and Line Tightening Specifications

Application | Specification
--- | ---
Metric | English
A/C Compressor Hose Support Strap Bolt | 8 N·m | 71 lb in
A/C Compressor/Condenser Hose Bracket Bolt | 8 N·m | 71 lb in
A/C Condenser Line Bolt | 27 N·m | 20 lb ft
Accessory Drive Belt Tensioner Bolt | 40 N·m | 30 lb ft
AIR Crossover Pipe Bushing Nut | 12 N·m | 108 lb in
AIR Crossover Pipe Support Bracket (Generator Bolt) Nut | 40 N·m | 30 lb ft
AIR Pipe Bolt | 20 N·m | 15 lb ft
Camshaft Bearing Cap Bolt | 8 N·m | 71 lb in
Camshaft Cover Bolt | 8 N·m | 71 lb in
Camshaft Sprocket Bolt

- First Pass

50 N·m

37 lb ft

- Second Pass

60 Degrees

60 Degrees

- Final Pass

15 Degrees

15 Degrees

Catalytic Converter Hanger Bolt | 20 N·m | 15 lb ft
Catalytic Converter Nut | 25 N·m | 18 lb ft
Coolant Pipe/Engine Lift Bracket Bolt | 20 N·m | 15 lb ft
Crankshaft Balancer Bolt | 20 N·m | 15 lb ft
Crankshaft Drive Gear Bolt

- First Pass

250 N·m

184 lb ft

- Second Pass

45 Degrees

45 Degrees

- Final Pass

15 Degrees

15 Degrees

Cylinder Head Bolt

- First Pass

25 N·m

18 lb ft

- Second Pass

90 Degrees

90 Degrees

- Third Pass

90 Degrees

90 Degrees

- Fourth Pass

90 Degrees

90 Degrees

- Fifth Pass

15 Degrees

15 Degrees

- Final Pass

15 Degrees

15 Degrees

Drive Belt Tensioner Bolt | 40 N·m | 30 lb ft
Engine Mount Lower Nut | 55 N·m | 41 lb ft
Engine Mount Upper Nut | 40 N·m | 30 lb ft
Engine Splash Shield Bolt | 10 N·m | 89 lb in
Engine Rear Cover Bolt | 8 N·m | 71 lb in
Engine Rear Cover Threaded Pin | 10 N·m | 89 lb in
Flywheel Bolt

- First Pass

65 N·m

48 lb ft

- Second Pass

30 Degrees

30 Degrees

- Final Pass

15 Degrees

15 Degrees

Front Timing Belt Cover Bolt | 8 N·m | 71 lb in
Generator Mounting Bolt (Lower) | 35 N·m | 26 lb ft
Generator Mounting Bolt (Upper) | 40 N·m | 30 lb ft
Idler Arm Bolt | 60 N·m | 44 lb ft
Intake Manifold Bolt | 20 N·m | 15 lb ft
Intake Manifold Spacer Bolt | 20 N·m | 15 lb ft
Intake Plenum Bolt | 20 N·m | 15 lb ft
Lower Oil Pan Bolt | 8 N·m | 71 lb in
Oil Baffle Bolt | 8 N·m | 71 lb in
Oil Cooler Cover Bolt | 30 N·m | 22 lb ft
Oil Cooler Inlet and Outlet Bolt | 20 N·m | 15 lb ft
Oil Filter Cartridge Housing Drain Plug | 10 N·m | 89 lb in
Oil Filter Cartridge Housing to Engine Block | 45 N·m | 33 lb ft
Oil Filter Cartridge Plastic Cap to Housing | 25 N·m | 18 lb ft
Oil Intake Pipe Bolt | 8 N·m | 71 lb in
Oil Pan Drain Plug | 10 N·m | 89 lb in
Oil Pump Bolt | 20 N·m | 15 lb ft
Power Steering Pump Pulley Bolt | 20 N·m | 15 lb ft
Throttle Body Bolt | 12 N·m | 106 lb in
Timing Belt Idler Pulley Bolt | 40 N·m | 30 lb ft
Timing Belt Tensioner Bracket Bolt | 40 N·m | 30 lb ft
Timing Belt Tensioner Pulley Nut | 20 N·m | 15 lb ft
Transmission to Upper Oil Pan Bolt | 40 N·m | 30 lb ft
Upper Oil Pan Bolt | 15 N·m | 11 lb ft
Water Crossover Bolt | 30 N·m | 22 lb ft
Water Pump Bolt | 25 N·m | 18 lb ft
Water Pump Pulley Bolt | 8 N·m | 71 lb in
Wiring Harness Channel Bolt | 8 N·m | 71 lb in

#### Hose and Line Tightening Specifications

Application | Specification
--- | ---
Metric | English
Engine Oil Cooler Line | 30 N·m | 22 lb ft
Fuel Return Hose to Fuel Rail | 15 N·m | 11 lb ft
Fuel Supply Hose to Fuel Rail | 15 N·m | 11 lb ft
Oil Cooler Feed and Return Lines to Engine Block | 30 N·m | 22 lb ft
Power Steering Pump Discharge Hose to Pump | 28 N·m | 21 lb ft