For 1990-2009 cars

### Removal Procedure

1. Remove the main case oil pan and filter. Refer to Changing Fluid and Oil Filter .
2. Disconnect the electrical connector from solenoid valve.
3. Pull out the retaining pin (2). Use pliers to pull pin out.
4. Remove the solenoid valve (2).

### Installation Procedure

1. Install the solenoid valve (2).
2. Install the retaining pin (1). Use a soft mallet to drive pin in.
3. Connect the electrical connector.
4. Install the oil pan and filter. Refer to Changing Fluid and Oil Filter .