For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rubber protective cover from the fog and cornering lamp.

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

3. Separate the fog lamp bulb/socket fastening tangs.
4. Remove the fog lamp bulb/socket from the fog lamp.
5. Disconnect the electrical connector from the fog lamp bulb/socket.

### Installation Procedure

1. Connect the electrical connector to the fog lamp bulb/socket.
2. Install the fog lamp bulb/socket to the fog lamp.
3. Engage the retaining tangs to secure the fog lamp bulb/socket to the fog lamp.
4. Install the rubber protective cover to the fog and cornering lamp.
5. Lower the vehicle.