For 1990-2009 cars

Drain hoses are pushed on and not clamped or cemented. Use caution when cleaning the channel and hose not to disconnected from the channel while cleaning.

1. Slide the sunscreen all the way rearward.
2. Place the glass panel to the fully open position, so that the front drain channels are in full view.
3. Front right and left drain channels can be checked and cleaned.
4. To access rear drain channels remove sunroof actuator. Refer to Sunroof Actuator Replacement