For 1990-2009 cars

1. Remove the cruise control cable from the heater hose clip (2).
2. Open the cable adjusting lever (1).
3. Slide the cable (1) together or apart in order to adjust the vertical endplay:

Specification
Vertical endplay (minimal deflection): 2.0 to 4.0 mm (0.08 to 0.16 in)

4. Close the adjusting lever (1).
5. Verify the cruise control system operation.

Install the cruise control cable to the heater hose clip (2).