For 1990-2009 cars

### Removal Procedure

Caution: When a rear compartment lid hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Open the rear compartment lid.
2. Remove the wiring and the shield (1) on the left side of the compartment lid hinge.
3. Remove the rear compartment lid strut. Refer to Rear Compartment Lid Strut Replacement
4. Remove the nuts (2) from the compartment lid upper hinge.
5. Remove the hinge screws (3) from the quarter panel.
6. Remove the rear compartment lid hinge (4).

### Installation Procedure

1. Install the rear compartment lid hinge (4).
2. Install the hinge screws (3) to the quarter panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the rear compartment lid hinge screws to 29 N·m (21 lb ft).

3. Install the nuts (2) to the rear compartment lid hinge (4).

Tighten
Tighten the rear compartment lid hinge nuts to 29 N·m (21 lb ft).

4. Install the rear compartment lid strut. Refer to Rear Compartment Lid Strut Replacement
5. Install the wiring and shield (1) to the left side compartment lid hinge.
6. Close the rear compartment lid.
7. Adjust rear compartment lid. Refer to Rear Compartment Lid Adjustment