For 1990-2009 cars

### Removal Procedure

1. Open the doors.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Drill out the 2 rocker corner molding rivets. The rocker molding does not need to be removed to replace the rocker corner molding.
5. Remove the rear corner molding.

### Installation Procedure

1. Push the rear corner molding into the rocker molding to lock in place.
2. Install the rocker corner molding rivets.
3. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Lower the vehicle.
5. Close the doors.