For 1990-2009 cars

Table 1: | Cruise Control Module Connector
Table 2: | Cruise Control Release Switch
Table 3: | Cruise Control Switch Connector

#### Cruise Control Module Connector

Connector Part Information |

• | 12065425

• | ASM 10F M/P 150 (BLACK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/RED | FA300 | Cruise control switch OFF input
B | BLK/YEL | FB300 | Cruise control switch SET/ACCEL input
C | BLK/BRN | FX500 | Cruise control switch RESUME/DECEL input
D | BLK/BLU | FP500 | Release switch disengage input
E | BLK | F500 | Ground
F | BRN | X500 | Fuse power to moduel - innition 1
G | BLK/WHT | FB500 | Stop lamp switch input
H | BRN/WHT | XM301 | Diagnostic serial data link input/output
J | BRN/BLU | XP950 | Engaged output - indicator bulb control
K | BLU/RED | PA500 | Vehicle speed input

#### Cruise Control Release Switch

Connector Part Information | F 2-34
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK/BLU | FB711 | Cruise release signal
2 | BLK/YEL | FP500 | Cruise release signal

#### Cruise Control Switch Connector

Connector Part Information | ZPF 4-50
--- | ---
Pin | Wire Color | Circuit No. | Function
A | BLK/RED | FA300 | Provides ON/OFF switch input to CRCONT module
B | BRN | X501 | Power input
C | BLK/BRN | FX500 | Provides RESUME/DECEL input to CRCONT module
D | BLK/BLK | F300 | Provides SET/ACCEL input to CRCONT module