For 1990-2009 cars

The rear compartment lid struts are not adjustable. Replace the rear compartment lid struts if damaged and/or leaking. Replace only one rear compartment lid strut at a time.

### Removal Procedure

Caution: When a rear compartment lid hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Support the rear compartment lid.
2. Lift up the retainer clips on the strut ends.
3. Remove the rear compartment lid strut from the hinge.
4. Repeat step 1 through step 3 to remove the other rear compartment lid strut.

### Installation Procedure

1. Install the rear compartment lid strut to the hinge.
2. Push in on the rear compartment lid strut until it locks in place.
3. Remove the support from the rear compartment lid.
4. Repeat steps 1 through 3 to install the other rear compartment lid strut.