For 1990-2009 cars

## Compressor Control Valve Assembly Install V5 - Direct Mount

#### Tools Required

J 41790-A Compressor Holding Fixture

1. Coat the control valve O-rings with clean 525 viscosity refrigeration oil.
2. Push the compressor control valve into the compressor with thumb pressure.
3. Using internal snap ring pliers, install the compressor control valve retaining ring.

Ensure that the retaining ring is properly seated in the ring groove.

4. Remove the compressor from the J 41790-A .