For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the exhaust muffler heat shields. Refer to Exhaust Heat Shield Replacement in Exhaust System.
3. Remove the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement in Propeller Shaft.
4. Measure the length of the exposed shaft thread from the nut to the end of the shaft.
5. Record the measurement.
6. Remove the rear parking brake shoe adjuster nut (1) from the rear parking brake lever shaft (2).

Important: Clean and lubricate the exposed threads of the shaft before attempting to turn the adjuster nut.

7. Remove the rear parking brake cable guide from the rear parking brake lever shaft.
8. Remove the parking brake cable adjuster link boot (2) from the rear parking brake lever shaft (1).
9. Lower the vehicle.
10. Remove the upper section of the center console. Refer to Console Replacement in Instrument Panel, Gages and Console.
11. Remove the rear parking brake lever bolts (1) from the lever.
12. Slightly lift the lever assembly from the underbody.
13. Remove the wiring harness connector (1) from the rear parking brake switch (2).
14. Remove the lever from the vehicle.
15. Remove the rear parking brake switch bolt (1) from the rear parking brake indicator switch (2).
16. Remove the parking brake switch from the lever.

### Installation Procedure

1. Install the parking brake switch to the lever.
2. Install the rear parking brake switch bolt (1) to the rear parking brake indicator switch (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the rear parking brake switch bolt (1) to 3 N·m (27 lb in).

3. Install the wiring harness connector (1) to the rear parking brake switch (2).
4. Install the parking brake lever to the vehicle.
5. Install the parking brake lever bolts (1) to the lever assembly.

Tighten
Tighten the parking brake lever bolts (1) to 20 N·m (15 lb ft).

6. Install the rear section of the center console. Refer to Console Replacement in Instrument Panel, Gages and Console.
7. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
8. Install the parking brake cable adjuster link boot (2) to the rear parking brake lever shaft (1).
9. Install the rear parking brake cable guide onto the lever shaft.
10. Install the rear parking brake shoe adjuster nut (1) to the rear parking brake lever shaft (2).
11. Adjust the rear parking brake shoe adjuster nut (1) to the recorded measurement from the installation procedure.
12. Install the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement in Propeller Shaft.
13. Test the parking brake operation and the state of the adjustment.

Important: Ensure the rear wheels still turn on the 4th notch of the parking brake application. Ensure the rear wheels are tight on the 7th notch of the parking brake application. Refer to Parking Brake Lever Adjustment in this section if the system does not operate within this range.

14. Install the exhaust muffler heat shields. Refer to Exhaust Heat Shield Replacement in Exhaust System.
15. Lower the vehicle.