For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Terminal Nut (Generator) | 6 N·m | 53 lb in
Battery Cable Terminal Nut (Starter) | 13 N·m | 115 lb in
Battery Hold Down Bolt | 15 N·m | 11 lb ft
Generator Cooling Duct Screw | 1 N·m | 9 lb in
Generator Mounting Nut Lower/Upper | 40 N·m | 30 lb ft
Negative Battery Cable Bracket Bolt | 25 N·m | 18 lb ft
Negative Battery Cable Clamp Bolt | 6 N·m | 53 lb in
Positive Battery Cable Clamp Bolt | 6 N·m | 53 lb in
Starter Solenoid Terminal Nut | 4 N·m | 35 lb in