For 1990-2009 cars

• | DSPL (1) -- Pressing this button will display either the time of day or the current station being played.

• | Preset Stations (2) -- The six preset buttons can be preset for up to 18 stations, 6 each of the AM, FM1, and FM2 bands. Preset the stations as follows:

- | Select the desired band using the BAND button.

- | Tune to the desired station.

- | Press and hold one of the six preset buttons until a chime sounds. (The display channel number and the audio will return.)

- | Holding the button for longer than two seconds will activate the fast seek mode.

• | FADE (3)

- | Lightly press the knob in order to extend outward.

- | Turn the knob clockwise or counterclockwise in order to move the sound to the RH or LH speakers.

- | The middle knob position is a detent and balances the speakers.

• | BAL (4)

- | Lightly press the knob in order to extend outward.

- | Turn the knob clockwise or counterclockwise in order to move the sound to the RH or LH speakers.

- | The middle knob position is a detent and balances the speakers.

• | SCAN (5)

- | Press and hold this button for 2-3 seconds or until the display shows PSCAN.

- | Each of the presets will be scanned for a few seconds and will continue until the button is pressed again.

• | TREBLE (6)

- | Lightly press the knob in order to extend outward.

- | Rotate the knob clockwise or counterclockwise in order to increase or decrease the treble response of the music.

• | TUNE/SEEK (7)

- | Press this button until a chime is heard in order to tune to the next higher or lower frequency.

- | If the button is held for more than two seconds after the chime, the radio will go into the fast tune mode.

- | Release the button when the desired station is reached.

• | BASS (8)

- | Lightly press the knob in order to extend outward.

- | Rotate the knob clockwise or counterclockwise in order to increase or decrease the bass response of the music.

• | BAND (9)

- | Press up for access to the FM1 and FM2 bands.

- | Press down for access to the AM band.

• | PWR/VOL Knob (10)

- | Press the volume knob in order to turn the radio ON or OFF.

- | Turn the knob clockwise/counterclockwise in order to turn the volume up or down. The knob is designed to turn infinitely.

• | SOURCE 11 -- Press this button in order to toggle between the radio, cassette, and CD functions.

• | HR/MIN (Clock)

- | Press DSPL until the clock is displayed.

- | Press and hold HR or MIN until the time display begins to change.

- | Release the button when you reach the correct time.

- | There is a two second delay before the clock goes into the time-set mode.