For 1990-2009 cars

### Removal Procedure

1. Remove the front door assist handle and molding. Refer to Assist Handle and Molding Replacement - Front Door .
2. Remove the mirror screws.
3. Remove the mirror from the door.
4. Disconnect the outside rearview mirror electrical connector.

### Installation Procedure

1. Connect the mirror electrical connector.
2. Install the mirror to the door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the mirror screws.

Tighten
Tighten the mirror screws to 10 N·m (89 lb in).

4. Install the front door assist handle and molding. Refer to Assist Handle and Molding Replacement - Front Door .