For 1990-2009 cars

### Heated Seat Switch

#### Removal Procedure

1. Remove the cover from the radio trim bezel.
2. Remove the heated seat switch cover by gently prying up on corner, access from the open hole where the radio trim bezel screw cover is placed.
3. Remove the heated seat switch from the instrument panel accessary trim panel by depressing both tabs locking tabs and remove switch.

### Installation Procedure

1. Install the heated seat switch to the instrument panel accessary trim panel.
2. Install the heated seat switch cover to the switch.
3. Install the screw cover to the radio trim bezel.

### Fuel Door Switch

#### Removal Procedure

Remove the fuel door release switch from the instrument panel accessary trim panel by prying gently on the right side of the switch.

### Installation Procedure

Install the fuel door release to the instrument panel accessary trim panel.

### Trunk Release Switch

#### Removal Procedure

Remove the trunk release switch from the instrument panel accessary trim panel by prying gently on the left side of the switch.

### Installation Procedure

Install the trunk release to the instrument panel accessary trim panel.