For 1990-2009 cars

## Applique Trim Panel Replacement Front Door

### Removal Procedure

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in Restraints.
2. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the three retaining clips from the plastic studs on the trim panel woodgrain applique.
4. Remove the applique.

### Installation Procedure

1. Install the applique.
2. Press the clips over the studs.
3. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in Restraints.

## Applique Trim Panel Replacement Rear Door

### Removal Procedure

1. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the three clips holding the trim panel woodgrain applique using a screwdriver.
3. Remove the applique.

### Installation Procedure

1. Install the applique.
2. Install the three clips using a screwdriver.
3. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .