For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the front seat cushion cover. Refer to Front Seat Cushion Replacement .
3. Remove seat cushion heater element:

3.1. | Cut along the seams on the inside of the seat cover. Do NOT cut through the front side of the seat cover.

3.2. | Cut the heater element electrical wiring.

3.3. | Remove the heater element and the wiring from the seat cover.

### Installation Procedure

1. Install the heating element for the front seat cushion to the seat cover.
2. Install the electrical wiring for the seat cushion heater element to the original position of the old wiring harness.
3. Place the old heating element on top of the new heating element.
4. Fold over the ends of the new heater element and tape the element to the seat cushion cover.
5. Install the front seat cushion cover. Refer to Front Seat Cushion Replacement .
6. Install the front seat. Refer to Driver and Passenger Seat Replacement .