For 1990-2009 cars

### Removal Procedure

1. Remove the RF floor air outlet. Refer to Floor Air Outlet Duct Replacement - Right Side
2. Remove the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
3. Bend downward at the accordion section of the duct in order to remove the duct from the side air vent.

### Installation Procedure

1. Install the floor duct:

• | Insert the duct into the module.

• | Bend at the accordion section in order to install.

2. Install the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
3. Install the RF floor air outlet. Refer to Floor Air Outlet Duct Replacement - Right Side