For 1990-2009 cars

### Conditions for Setting the DTC

This code is set when the vehicle's battery voltage momentarily goes above 16.0 V.

### Action Taken When the DTC Sets

The detection of leveling output, and the position out-of-range malfunctions are disabled. This is necessary to prevent erroneous detection of malfunction conditions due to engine crank or unusual system voltage conditions.

### Conditions for Clearing the DTC

• | The DTC will clear when battery voltage returns to its nominal range.

• | Using a scan tool.

### Diagnostic Aids

• | The battery system should be checked for proper functionality.

• | This code does not require the replacing of the Automatic Level Control (ALC) sensor.

• | This code will not cause the LEVELING indicator lamp to flash.

• | Make sure that the automatic leveling control sensor is receiving the correct voltage.

• | Make sure that the ALC sensor has a good ground.