For 1990-2009 cars

### Removal Procedure

1. Remove the assist handle and cover. Refer to Assist Handle and Molding Replacement - Rear Door .
2. Disconnect the power window switch connector.
3. Snap out the switch.

### Installation Procedure

1. Snap on the switch.
2. Connect the switch connector.
3. Install the assist handle and cover. Refer to Assist Handle and Molding Replacement - Rear Door .