For 1990-2009 cars

#### Rear Axle Specifications

Application | Specification
--- | ---
Metric | English
Ring Gear Diameter | 188 mm | lb 7.401 in
Axle Type | Rididly Mounted Housing, Non-Locking
Gear Type | Hypoid
Gear Ratio | 3.90:1
Number of Ring Gear Teeth | 39
Number of Drive Pinion Gear Teeth | 10
ABS Sensor Air Gap | 0.13-1.0 mm | lb 0.005-0.039 in
Ring Gear to Drive Pinion Backlash | 0.10-0.20 mm | lb 0.004-0.008 in