For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Disconnect the windshield wiper/washer switch.
2. Use a DMM in order to measure the resistance between terminal 53A and terminal W of the windshield wiper/washer switch while holding the mist switch in the ON position.

Is the measured resistance within the specified range?

Less than 5 ohms

Go to Step 3

Go to Step 4

3 |

1. Locate an open or a high resistance in CKT FA4.
2. Repair the open or the high resistance in CKT FA4.

Is the repair complete?

--

Go to Step 5

--

4 | Replace the windshield wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement - On Vehicle in Steering. Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Reconnect all of the components and the connectors that were disconnected.
2. Verify that the windshield washer pump and the windshield wipers operate properly when the windshield wiper/washer switch is in the MIST position.

Do the windshield washer pump and the windshield wipers operate properly?

--

Go to Wiper/Washer System Check

Go to Step 1