For 1990-2009 cars

### Removal Procedure

1. Loosen the set screw (1).
2. Release the locking tabs in order to remove the ignition switch (2) from the lock housing (3).

### Installation Procedure

Press the ignition switch towards the rear of the column until the locking tabs are fully engaged in order to install the ignition switch (1) onto the lock housing (2).

Tighten
Tighten the set screw onto the lock housing (2).