For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
4. Remove the bellcrank center plastic pin, using a small punch.
5. Remove the bellcrank from the retainer.
6. Remove the lock rod from the bellcrank.

### Installation Procedure

1. Install the bellcrank lock rod.
2. Install the bellcrank to the retainer.
3. Install the bellcrank center plastic pin into the retainer by pushing inward.
4. Install the inside door handle. Refer to Refer to Rear Side Door Inside Handle Replacement .
5. Install the door water deflector. Refer to Rear Side Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .