For 1990-2009 cars

# SMU - OB - MAINTENANCE AND LUBRICATION - REVISED

#### SUBJECT: SMU - SECTION OB - MAINTENANCE AND LUBRICATION - REVISED ENGINE OIL CAPACITY

#### MODELS: 1997 CADILLAC CATERA

THE ENGINE OIL CAPACITY INFORMATION ON PAGE OB-1 OF THE PRELIMINARY CATERA SERVICE MANUAL IS INCORRECT. THE CORRECT INFORMATION IS AS FOLLOWS:

ENGINE OIL WITH FILTER CHANGE 6.1 QUARTS(5.75L)

ENGINE OIL WITHOUT FILTER CHANGE 5.8 QUARTS(5.5L)

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.