For 1990-2009 cars

1. Remove the second and third clutch assembly by lifting up on the input shaft.
2. Remove the reverse clutch cushion plate (614).
3. Remove the reverse clutch plates (615-616) from the second clutch drum
4. Inspect the reverse clutch composition plates (616) for:

• | damaged tangs

• | delamination

• | excessive wear

5. Inspect the reverse clutch steel plates (615) for:

• | worn lugs

• | heat damage

6. Remove the reverse clutch pressure plate (617).