For 1990-2009 cars

1. Inspect the shift control cable for the following conditions. Repair or replace as needed:

• | Wear at the pivot points

• | Bent or broken cable housing

2. Inspect all of the seals, the gaskets, the O-ring seals, and the mating surfaces for the following conditions. Replace as needed:

• | Nicks

• | Cuts

• | Damage

3. Inspect the snap rings for the following conditions. Replace as needed:

• | Expansion

• | Compression

• | Distortion

• | Nicks

• | Improper ring to groove fit

4. Inspect all of the bearing and thrust surfaces for the following conditions. Replace as needed:

• | Wear

• | Scoring

• | Pitting