For 1990-2009 cars

### Removal Procedure

1. Remove the mirror lens. Refer to Outside Rearview Mirror Glass Replacement .
2. Disconnect the outside rearview motor connector.
3. Remove the motor screws.
4. Remove the motor.

### Installation Procedure

1. Install the motor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the motor screws.

Tighten
Tighten the outside rearview motor screws until fully seated but not stripped.

3. Connect the motor connector.
4. Install the mirror lens. Refer to Outside Rearview Mirror Glass Replacement .