For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seatback cushion. Refer to Rear Seat Back Replacement .
3. Remove the rear seatback release latch. Refer to Rear Seat Back Release Latch Replacement .
4. If equipped, remove the heating element wiring for the rear seatback from the seatback pad.
5. Remove the rear seatback cushion cover

5.1. | Unhook the rear seatback cushion cover from around the frame.

5.2. | Remove the retainer rings from the center of the rear seatback cushion cover.

### Installation Procedure

1. Install the heating element wiring for the rear seatback to the seatback pad, if equipped.
2. Install the rear seatback cushion cover:

2.1. | Install the retaining rings to the center of the rear seatback cushion cover.

2.2. | Install rear seatback cushion cover around the frame.

3. Install the rear seatback release latch. Refer to Rear Seat Back Release Latch Replacement .
4. Install the rear seatback cushion. Refer to Rear Seat Back Replacement .
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .