For 1990-2009 cars

## Emblem/Nameplate Replacement Rear Compartment Lid

### Removal Procedure

1. Hold a heat gun 152 mm (6 in) from the emblem or the nameplate and apply heat for about 30 seconds while moving the heat gun in a circular motion.
2. Use a flat-bladed tool in order to peel the emblem or the nameplate from the rear compartment lid. Do NOT damage the paint surface.
3. Clean the area using a suitable solvent of isopropyl alcohol 50/50 mixture by volume with water, or use a high-flash naphtha.

### Installation Procedure

1. The new emblem or the new nameplate must be 26°C (80°F) minimum, or 6°C (10°F) above the ambient air temperature, whichever is higher.

Do NOT exceed 40°C (105°F) during the installation procedure.

2. Remove the backing from the new emblem or the new nameplate.

Important: Position the emblem or the nameplate carefully on the vehicle. You will not be able to move the emblem or the nameplate after contact with the vehicle.

3. Press the emblem or the nameplate into place.
4. Apply constant pressure for 30 seconds.