For 1990-2009 cars

### Tools Required

• | J 38553 3-4 Accumulator Piston Installer

• | J 38559 Compressor

• | J 8059 Snap Ring Pliers

1. Install the accumulator piston seal (19).
2. Install the piston pin (17) into the piston (18).
3. Install J 38553 into the adapter case bore.
4. Push the fourth clutch accumulator piston (18) into position.
5. Remove J 38553 .
6. Install the fourth clutch accumulator piston spring (16).
7. Install the fourth clutch accumulator piston cover (14).
8. Install J 38559 onto the adapter case.

Notice: Do not over compress the spring or damage to the piston may occur.

9. Compress the accumulator piston spring (16).
10. Install the accumulator piston cover retainer ring (13) using J 8059 .
11. Remove J 38559 .