For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Loosen the power steering pump pulley bolts with the serpentine drive belt still attached.
3. Remove the serpentine drive belt. Refer to Drive Belt Replacement in Engine Mechanical.
4. Remove the power steering pump pulley bolts.
5. Remove the power steering pump pulley from the pump.

### Installation Procedure

1. Install the power steering pump pulley to the pump.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the power steering pump pulley bolts loosely.
3. Install the serpentine drive belt. Refer to Drive Belt Replacement in Engine Mechanical.

Tighten
Tighten the power steering pump pulley bolts to 20 N·m (15 lb ft).

4. Reconnect the negative battery cable.
5. Reprogram applicable accessories.