For 1990-2009 cars

Problem | Action
--- | ---
The power steering fluid is low. | Check and add power steering fluid, as necessary. Refer to Checking and Adding Power Steering Fluid .
Air is present in the power steering system. |

1. Inspect the power steering system for leaks and repair, as necessary. Refer to Power Steering Fluid Leaks .
2. Bleed the power steering system. Refer to Power Steering System Bleeding .