For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
4. Remove all the rods that attach to the lock assembly.
5. Remove the door lock actuator electrical connector.
6. Remove the door lock screws.
7. Remove the door lock.
8. Remove the door lock actuator screws.
9. Remove the door lock actuator from door lock.

### Installation Procedure

1. Install the door lock actuator to the door lock.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the door lock actuator screws.

Tighten
Tighten the door lock actuator screws to 3 N·m(27 lb in).

3. Install the door lock.
4. Install the door lock screws.

Tighten
Tighten the door lock screws to 8 N·m(71 lb in).

5. Install the door lock actuator electrical connector.
6. Install all the rods that attach to the lock assembly.
7. Install the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
8. Install the door water deflector. Refer to Rear Side Door Water Deflector Replacement .
9. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .