For 1990-2009 cars

### Removal Procedure

1. Remove the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
2. Disconnect the blower control module electrical connector.
3. Disconnect the blower motor electrical connector.
4. Release the blower control module retainer tabs.
5. Remove the blower control module from the blower motor housing.

### Installation Procedure

1. Position the blower control module to the blower motor housing.
2. Connect the blower control module retainer tabs.

Ensure the retainer tabs are fully seated.

3. Connect the blower motor electrical connector.
4. Connect the blower control module electrical connector.
5. Install the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.