For 1990-2009 cars

## Drive Belt Tensioner Installation Serpentine

1. Install the drive belt tensioner to the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the drive belt tensioner bolts.

Tighten
Tighten the drive belt tensioner bolts to 40 N·m (30 lb ft).

3. Route the drive belt over all except the water pump pulleys.
4. Use a wrench on the center bolt of the drive belt tensioner pulley (5) and rotate downward.

Route the drive belt over the water pump pulley.

5. Tighten the water pump pulley bolts.

Tighten
Tighten the water pump pulley bolts to 8 N·m (71 lb in).

6. Tighten the power steering pump pulley bolts.

Tighten
Tighten the power steering pump pulley bolts to 20 N·m (15 lb ft).