For 1990-2009 cars

### Removal Procedure

1. Remove the speaker grill cover from the door assist handle molding using a flat-tipped screwdriver.
2. Remove the door assist handle molding from the door panel using a flat tipped screwdriver.
3. Disconnect the electrical connector from the speaker.
4. Remove the speaker.

### Installation Procedure

1. Install the speaker into the door assist handle molding.
2. Connect the electrical connector to the speaker.
3. Install the door assist handle molding into the door panel.
4. Align and snap the speaker grill into the door assist handle molding.
5. Verify speaker operation.